[directories](!)
astetcdir => /etc/asterisk
astmoddir => /usr/lib/asterisk/modules
astvarlibdir => /var/lib/asterisk
astdbdir => /var/lib/asterisk
astkeydir => /var/lib/asterisk
astdatadir => /var/lib/asterisk
astagidir => /var/lib/asterisk/agi-bin
astspooldir => /var/spool/asterisk
astrundir => /var/run/asterisk
astlogdir => /var/log/asterisk

[options]
;verbose = 3
;debug = 3
;alwaysfork = yes		; Same as -F at startup.
;nofork = yes			; Same as -f at startup.
;quiet = yes			; Same as -q at startup.
;timestamp = yes		; Same as -T at startup.
;execincludes = yes		; Support #exec in config files.
;console = yes			; Run as console (same as -c at startup).
;highpriority = yes		; Run realtime priority (same as -p at
				; startup).
;initcrypto = yes		; Initialize crypto keys (same as -i at
				; startup).
;nocolor = yes			; Disable console colors.
;dontwarn = yes			; Disable some warnings.
;dumpcore = yes			; Dump core on crash (same as -g at startup).
;languageprefix = yes		; Use the new sound prefix path syntax.
;internal_timing = yes
;systemname = my_system_name	; Prefix uniqueid with a system name for
				; Global uniqueness issues.
;autosystemname = yes		; Automatically set systemname to hostname,
				; uses 'localhost' on failure, or systemname if
				; set.
;maxcalls = 10			; Maximum amount of calls allowed.
;maxload = 0.9			; Asterisk stops accepting new calls if the
				; load average exceed this limit.
;maxfiles = 1000		; Maximum amount of openfiles.
;minmemfree = 1			; In MBs, Asterisk stops accepting new calls if
				; the amount of free memory falls below this
				; watermark.
;cache_record_files = yes	; Cache recorded sound files to another
				; directory during recording.
;record_cache_dir = /tmp	; Specify cache directory (used in conjunction
				; with cache_record_files).
;transmit_silence = yes		; Transmit silence while a channel is in a
				; waiting state, a recording only state, or
				; when DTMF is being generated.  Note that the
				; silence internally is generated in raw signed
				; linear format. This means that it must be
				; transcoded into the native format of the
				; channel before it can be sent to the device.
				; It is for this reason that this is optional,
				; as it may result in requiring a temporary
				; codec translation path for a channel that may
				; not otherwise require one.
;transcode_via_sln = yes	; Build transcode paths via SLINEAR, instead of
				; directly.
;runuser = asterisk		; The user to run as.
;rungroup = asterisk		; The group to run as.
;lightbackground = yes		; If your terminal is set for a light-colored
				; background.
documentation_language = en_US	; Set the language you want documentation
				; displayed in. Value is in the same format as
				; locale names.
;hideconnect = yes		; Hide messages displayed when a remote console
				; connects and disconnects.
;lockconfdir = no		; Protect the directory containing the
				; configuration files (/etc/asterisk) with a
				; lock.

; Changing the following lines may compromise your security.
;[files]
;astctlpermissions = 0660
;astctlowner = root
;astctlgroup = apache
;astctl = asterisk.ctl

[compat]
pbx_realtime=1.6
res_agi=1.6
app_set=1.6
