;
; SIP Configuration example for Asterisk
;
; SIP dial strings
;-----------------------------------------------------------
; In the dialplan (extensions.conf) you can use several 
; syntaxes for dialing SIP devices.
;	SIP/devicename
;	SIP/username@domain   (SIP uri)
;	SIP/username[:password[:md5secret[:authname]]]@host[:port]
;	SIP/devicename/extension
;
;
; Devicename
;      devicename is defined as a peer in a section below.
;
; username@domain
; 	Call any SIP user on the Internet
;	(Don't forget to enable DNS SRV records if you want to use this)
; 
; devicename/extension
; 	If you define a SIP proxy as a peer below, you may call
; 	SIP/proxyhostname/user or SIP/user@proxyhostname 
; 	where the proxyhostname is defined in a section below 
;	This syntax also works with ATA's with FXO ports
;
; SIP/username[:password[:md5secret[:authname]]]@host[:port]
;	This form allows you to specify password or md5secret and authname
;	without altering any authentication data in config.
;	Examples:
;
;	SIP/*98@mysipproxy
;	SIP/sales:topsecret::account02@domain.com:5062
;	SIP/12345678::bc53f0ba8ceb1ded2b70e05c3f91de4f:myname@192.168.0.1
;
; All of these dial strings specify the SIP request URI.
; In addition, you can specify a specific To: header by adding an
; exclamation mark after the dial string, like
;
; 	SIP/sales@mysipproxy!sales@edvina.net
;
; CLI Commands
; -------------------------------------------------------------
; Useful CLI commands to check peers/users:
;   sip show peers		Show all SIP peers (including friends)
;   sip show users		Show all SIP users (including friends)
;   sip show registry		Show status of hosts we register with
;
;   sip set debug		Show all SIP messages
;
;   sip reload			Reload configuration file
;				Active SIP peers will not be reconfigured
;

; ** Deprecated configuration options **
; The "call-limit" configuation option is deprecated. It still works in
; this version of Asterisk, but will disappear in the next version.
; You are encouraged to use the dialplan groupcount functionality
; to enforce call limits instead of using this channel-specific method.
;
; You can still set limits per device in sip.conf or in a database by using 
; "setvar" to set variables that can be used in the dialplan for various limits.

[general]
context=default			; Default context for incoming calls
;allowguest=no			; Allow or reject guest calls (default is yes)
;match_auth_username=yes	; if available, match user entry using the
				; 'username' field from the authentication line
				; instead of the From: field.
;;
;; hash table sizes. For maximum efficiency, adjust the following
;; values to be slightly larger than the maximum number of users/peers.
;; Too large, and space is wasted. Too small, and things will run slower.
;; 563 is probably way too big for small (home) applications, but it
;; should cover most small/medium sites.
;; it is recommended to make the sizes be a prime number!
;; This was internally set to 17 for small-memory applications...
;; All tables default to 563, except when compiled in LOW_MEMORY mode,
;; in which case, they default to 17. You can override this by uncommenting
;; the following, and changing the values.
;hash_users=563
;hash_peers=563
;hash_dialogs=563

allowoverlap=no			; Disable overlap dialing support. (Default is yes)
;allowtransfer=no		; Disable all transfers (unless enabled in peers or users)
				; Default is enabled
;realm=mydomain.tld		; Realm for digest authentication
				; defaults to "asterisk". If you set a system name in
				; asterisk.conf, it defaults to that system name
				; Realms MUST be globally unique according to RFC 3261
				; Set this to your host name or domain name
bindport=5060			; UDP Port to bind to (SIP standard port is 5060)
				; bindport is the local UDP port that Asterisk will listen on
bindaddr=0.0.0.0		; IP address to bind to (0.0.0.0 binds to all)

;
; Note that the TCP and TLS support for chan_sip is currently considered
; experimental.  Since it is new, all of the related configuration options are
; subject to change in any release.  If they are changed, the changes will
; be reflected in this sample configuration file, as well as in the UPGRADE.txt file.
;
tcpenable=yes                   ; Enable server for incoming TCP connections (default is yes)
tcpbindaddr=0.0.0.0	        ; IP address for TCP server to bind to (0.0.0.0 binds to all interfaces)
                                ; Optionally add a port number, 192.168.1.1:5062 (default is port 5060)

;tlsenable=no                   ; Enable server for incoming TLS (secure) connections (default is no)
;tlsbindaddr=0.0.0.0            ; IP address for TLS server to bind to (0.0.0.0) binds to all interfaces)
                                ; Optionally add a port number, 192.168.1.1:5063 (default is port 5061)
				; Remember that the IP address must match the common name (hostname) in the
				; certificate, so you don't want to bind a TLS socket to multiple IP addresses.

;tlscertfile=asterisk.pem	; Certificate file (*.pem only) to use for TLS connections 
			 	; default is to look for "asterisk.pem" in current directory

;tlscafile=</path/to/certificate>
;	If the server your connecting to uses a self signed certificate
;	you should have their certificate installed here so the code can 
;	verify the authenticity of their certificate.

;tlscadir=</path/to/ca/dir>
;	A directory full of CA certificates.  The files must be named with 
;	the CA subject name hash value. 
;	(see man SSL_CTX_load_verify_locations for more info) 

;tlsdontverifyserver=[yes|no]
;	If set to yes, don't verify the servers certificate when acting as 
;	a client.  If you don't have the server's CA certificate you can
;	set this and it will connect without requiring tlscafile to be set.
;	Default is no.

;tlscipher=<SSL cipher string>
;	A string specifying which SSL ciphers to use or not use
;	A list of valid SSL cipher strings can be found at: 
;		http://www.openssl.org/docs/apps/ciphers.html#CIPHER_STRINGS

srvlookup=yes			; Enable DNS SRV lookups on outbound calls
				; Note: Asterisk only uses the first host 
				; in SRV records
				; Disabling DNS SRV lookups disables the 
				; ability to place SIP calls based on domain 
				; names to some other SIP users on the Internet

;pedantic=yes			; Enable checking of tags in headers, 
				; international character conversions in URIs
				; and multiline formatted headers for strict
				; SIP compatibility (defaults to "no")

; See qos.tex or Quality of Service section of asterisk.pdf for a description of these parameters.
;tos_sip=cs3                    ; Sets TOS for SIP packets.
;tos_audio=ef                   ; Sets TOS for RTP audio packets.
;tos_video=af41                 ; Sets TOS for RTP video packets.
;tos_text=af41                  ; Sets TOS for RTP text packets.

;cos_sip=3                      ; Sets 802.1p priority for SIP packets.
;cos_audio=5                    ; Sets 802.1p priority for RTP audio packets.
;cos_video=4                    ; Sets 802.1p priority for RTP video packets.
;cos_text=3                     ; Sets 802.1p priority for RTP text packets.

;maxexpiry=3600			; Maximum allowed time of incoming registrations
				; and subscriptions (seconds)
;minexpiry=60			; Minimum length of registrations/subscriptions (default 60)
;defaultexpiry=120		; Default length of incoming/outgoing registration
;qualifyfreq=60                 ; Qualification: How often to check for the 
                                ; host to be up in seconds
                                ; Set to low value if you use low timeout for
                                ; NAT of UDP sessions
;notifymimetype=text/plain	; Allow overriding of mime type in MWI NOTIFY
;buggymwi=no			; Cisco SIP firmware doesn't support the MWI RFC
				; fully. Enable this option to not get error messages
				; when sending MWI to phones with this bug.
;vmexten=voicemail		; dialplan extension to reach mailbox sets the 
				; Message-Account in the MWI notify message 
				; defaults to "asterisk"
;disallow=all			; First disallow all codecs
;allow=ulaw			; Allow codecs in order of preference
;allow=ilbc			; see doc/rtp-packetization for framing options
;
; This option specifies a preference for which music on hold class this channel
; should listen to when put on hold if the music class has not been set on the
; channel with Set(CHANNEL(musicclass)=whatever) in the dialplan, and the peer
; channel putting this one on hold did not suggest a music class.
;
; This option may be specified globally, or on a per-user or per-peer basis.
;
;mohinterpret=default
;
; This option specifies which music on hold class to suggest to the peer channel
; when this channel places the peer on hold. It may be specified globally or on
; a per-user or per-peer basis.
;
;mohsuggest=default
;
;parkinglot=plaza		; Sets the default parking lot for call parking
				; This may also be set for individual users/peers
				; Parkinglots are configured in features.conf
;language=en			; Default language setting for all users/peers
				; This may also be set for individual users/peers
;relaxdtmf=yes			; Relax dtmf handling
;trustrpid = no			; If Remote-Party-ID should be trusted
;sendrpid = yes			; If Remote-Party-ID should be sent
;progressinband=never		; If we should generate in-band ringing always
				; use 'never' to never use in-band signalling, even in cases
				; where some buggy devices might not render it
				; Valid values: yes, no, never Default: never
;useragent=Asterisk PBX		; Allows you to change the user agent string
				; The default user agent string also contains the Asterisk
				; version. If you don't want to expose this, change the
				; useragent string.
;sdpsession=Asterisk PBX	; Allows you to change the SDP session name string, (s=)
				; Like the useragent parameter, the default user agent string
				; also contains the Asterisk version.
;sdpowner=root			; Allows you to change the username field in the SDP owner string, (o=)
				; This field MUST NOT contain spaces
;promiscredir = no      	; If yes, allows 302 or REDIR to non-local SIP address
	                       	; Note that promiscredir when redirects are made to the
       	                	; local system will cause loops since Asterisk is incapable
       	                	; of performing a "hairpin" call.
;usereqphone = no		; If yes, ";user=phone" is added to uri that contains
				; a valid phone number
;dtmfmode = rfc2833		; Set default dtmfmode for sending DTMF. Default: rfc2833
				; Other options: 
				; info : SIP INFO messages (application/dtmf-relay)
				; shortinfo : SIP INFO messages (application/dtmf)
				; inband : Inband audio (requires 64 kbit codec -alaw, ulaw)
				; auto : Use rfc2833 if offered, inband otherwise

;compactheaders = yes		; send compact sip headers.
;
;videosupport=yes		; Turn on support for SIP video. You need to turn this on
				; in the this section to get any video support at all.
				; You can turn it off on a per peer basis if the general
				; video support is enabled, but you can't enable it for
				; one peer only without enabling in the general section.
;maxcallbitrate=384		; Maximum bitrate for video calls (default 384 kb/s)
				; Videosupport and maxcallbitrate is settable
				; for peers and users as well
;callevents=no			; generate manager events when sip ua 
				; performs events (e.g. hold)
;authfailureevents=no		; generate manager "peerstatus" events when peer can't
				; authenticate with Asterisk. Peerstatus will be "rejected".
;alwaysauthreject = yes		; When an incoming INVITE or REGISTER is to be rejected,
 		    		; for any reason, always reject with '401 Unauthorized'
 				; instead of letting the requester know whether there was
 				; a matching user or peer for their request

;g726nonstandard = yes		; If the peer negotiates G726-32 audio, use AAL2 packing
				; order instead of RFC3551 packing order (this is required
				; for Sipura and Grandstream ATAs, among others). This is
				; contrary to the RFC3551 specification, the peer _should_
				; be negotiating AAL2-G726-32 instead :-(
;outboundproxy=proxy.provider.domain           ; send outbound signaling to this proxy, not directly to the devices
;outboundproxy=proxy.provider.domain:8080       ; send outbound signaling to this proxy, not directly to the devices
;outboundproxy=proxy.provider.domain,force      ; Send ALL outbound signalling to proxy, ignoring route: headers
;matchexterniplocally = yes     ; Only substitute the externip or externhost setting if it matches
                                ; your localnet setting. Unless you have some sort of strange network
                                ; setup you will not need to enable this.

;
; If regcontext is specified, Asterisk will dynamically create and destroy a
; NoOp priority 1 extension for a given peer who registers or unregisters with
; us and have a "regexten=" configuration item.  
; Multiple contexts may be specified by separating them with '&'. The 
; actual extension is the 'regexten' parameter of the registering peer or its
; name if 'regexten' is not provided.  If more than one context is provided,
; the context must be specified within regexten by appending the desired
; context after '@'.  More than one regexten may be supplied if they are 
; separated by '&'.  Patterns may be used in regexten.
;
;regcontext=sipregistrations
;regextenonqualify=yes		; Default "no"
				; If you have qualify on and the peer becomes unreachable
				; this setting will enforce inactivation of the regexten
				; extension for the peer
;
;--------------------------- SIP timers ----------------------------------------------------
; These timers are used primarily in INVITE transactions. 
; The default for Timer T1 is 500 ms or the measured run-trip time between
; Asterisk and the device if you have qualify=yes for the device.
;
;t1min=100			; Minimum roundtrip time for messages to monitored hosts
				; Defaults to 100 ms
;timert1=500		        ; Default T1 timer
				; Defaults to 500 ms or the measured round-trip
				; time to a peer (qualify=yes).
;timerb=32000		        ; Call setup timer. If a provisional response is not received
				; in this amount of time, the call will autocongest
				; Defaults to 64*timert1

;--------------------------- RTP timers ----------------------------------------------------
; These timers are currently used for both audio and video streams. The RTP timeouts
; are only applied to the audio channel.
; The settings are settable in the global section as well as per device
;
;rtptimeout=60			; Terminate call if 60 seconds of no RTP or RTCP activity
				; on the audio channel
				; when we're not on hold. This is to be able to hangup
				; a call in the case of a phone disappearing from the net,
				; like a powerloss or grandma tripping over a cable.
;rtpholdtimeout=300		; Terminate call if 300 seconds of no RTP or RTCP activity
				; on the audio channel
				; when we're on hold (must be > rtptimeout)
;rtpkeepalive=<secs>		; Send keepalives in the RTP stream to keep NAT open
				; (default is off - zero)

;--------------------------- SIP Session-Timers (RFC 4028)------------------------------------
; SIP Session-Timers provide an end-to-end keep-alive mechanism for active SIP sessions.
; This mechanism can detect and reclaim SIP channels that do not terminate through normal
; signaling procedures. Session-Timers can be configured globally or at a user/peer level.
; The operation of Session-Timers is driven by the following configuration parameters:
;
; * session-timers    - Session-Timers feature operates in the following three modes:
;                            originate : Request and run session-timers always
;                            accept    : Run session-timers only when requested by other UA
;                            refuse    : Do not run session timers in any case
;                       The default mode of operation is 'accept'.
; * session-expires   - Maximum session refresh interval in seconds. Defaults to 1800 secs.
; * session-minse     - Minimum session refresh interval in seconds. Defualts to 90 secs.
; * session-refresher - The session refresher (uac|uas). Defaults to 'uas'.
;
;session-timers=originate
;session-expires=600
;session-minse=90
;session-refresher=uas


;--------------------------- SIP DEBUGGING ---------------------------------------------------
;sipdebug = yes			; Turn on SIP debugging by default, from
				; the moment the channel loads this configuration
;recordhistory=yes		; Record SIP history by default 
				; (see sip history / sip no history)
;dumphistory=yes		; Dump SIP history at end of SIP dialogue
				; SIP history is output to the DEBUG logging channel


;--------------------------- STATUS NOTIFICATIONS (SUBSCRIPTIONS) ----------------------------
; You can subscribe to the status of extensions with a "hint" priority
; (See extensions.conf.sample for examples)
; chan_sip support two major formats for notifications: dialog-info and SIMPLE 
;
; You will get more detailed reports (busy etc) if you have a call counter enabled
; for a device. 
;
; If you set the busylevel, we will indicate busy when we have a number of calls that 
; matches the busylevel treshold.
;
; For queues, you will need this level of detail in status reporting, regardless
; if you use SIP subscriptions. Queues and manager use the same internal interface
; for reading status information.
;
; Note: Subscriptions does not work if you have a realtime dialplan and use the
; realtime switch.
;
;allowsubscribe=no		; Disable support for subscriptions. (Default is yes)
;subscribecontext = default	; Set a specific context for SUBSCRIBE requests
				; Useful to limit subscriptions to local extensions
				; Settable per peer/user also
;notifyringing = yes           ; Control whether subscriptions already INUSE get sent
                               ; RINGING when another call is sent (default: no)
;notifyhold = yes		; Notify subscriptions on HOLD state (default: no)
				; Turning on notifyringing and notifyhold will add a lot
				; more database transactions if you are using realtime.
;callcounter = yes		; Enable call counters on devices. This can be set per
				; device too.
;counteronpeer = yes		; Apply call counting on peers only. This will improve 
				; status notification when you are using type=friend
				; Inbound calls, that really apply to the user part
				; of a friend will now be added to and compared with
				; the peer counter instead of applying two call counters,
				; one for the peer and one for the user.
				; "sip show inuse" will only show active calls on 
				; the peer side of a "type=friend" object if this
				; setting is turned on.

;----------------------------------------- T.38 FAX PASSTHROUGH SUPPORT -----------------------
;
; This setting is available in the [general] section as well as in device configurations.
; Setting this to yes, enables T.38 fax (UDPTL) passthrough on SIP to SIP calls, provided
; both parties have T38 support enabled in their Asterisk configuration 
; This has to be enabled in the general section for all devices to work. You can then
; disable it on a per device basis. 
;
; T.38 faxing only works in SIP to SIP calls, with no local or agent channel being used.
;
; t38pt_udptl = yes            ; Default false
;
;----------------------------------------- OUTBOUND SIP REGISTRATIONS  ------------------------
; Asterisk can register as a SIP user agent to a SIP proxy (provider)
; Format for the register statement is:
;       register => [transport://]user[:secret[:authuser]]@host[:port][/extension][~expiry]
;
; 
;
; If no extension is given, the 's' extension is used. The extension needs to
; be defined in extensions.conf to be able to accept calls from this SIP proxy
; (provider).
;
; host is either a host name defined in DNS or the name of a section defined
; below.
;
; A similar effect can be achieved by adding a "callbackextension" option in a peer section.
; this is equivalent to having the following line in the general section:
;
;	register => username:secret@host/callbackextension
;
; and more readable because you don't have to write the parameters in two places
; (note that the "port" is ignored - this is a bug that should be fixed).
;
; Examples:
;
;register => 1234:password@mysipprovider.com	
;
;     This will pass incoming calls to the 's' extension
;
;
;register => 2345:password@sip_proxy/1234
;
;    Register 2345 at sip provider 'sip_proxy'.  Calls from this provider
;    connect to local extension 1234 in extensions.conf, default context,
;    unless you configure a [sip_proxy] section below, and configure a
;    context.
;    Tip 1: Avoid assigning hostname to a sip.conf section like [provider.com]
;    Tip 2: Use separate type=peer and type=user sections for SIP providers
;           (instead of type=friend) if you have calls in both directions
  
;registertimeout=20		; retry registration calls every 20 seconds (default)
;registerattempts=10		; Number of registration attempts before we give up
				; 0 = continue forever, hammering the other server
				; until it accepts the registration
				; Default is 0 tries, continue forever

;----------------------------------------- NAT SUPPORT ------------------------
;
; WARNING: SIP operation behind a NAT is tricky and you really need
; to read and understand well the following section.
;
; When Asterisk is behind a NAT device, the "local" address (and port) that
; a socket is bound to has different values when seen from the inside or
; from the outside of the NATted network. Unfortunately this address must
; be communicated to the outside (e.g. in SIP and SDP messages), and in
; order to determine the correct value Asterisk needs to know:
;
; + whether it is talking to someone "inside" or "outside" of the NATted network.
;   This is configured by assigning the "localnet" parameter with a list
;   of network addresses that are considered "inside" of the NATted network.
;   IF LOCALNET IS NOT SET, THE EXTERNAL ADDRESS WILL NOT BE SET CORRECTLY.
;   Multiple entries are allowed, e.g. a reasonable set is the following:
;
;      localnet=192.168.0.0/255.255.0.0 ; RFC 1918 addresses
;      localnet=10.0.0.0/255.0.0.0	; Also RFC1918
;      localnet=172.16.0.0/12		; Another RFC1918 with CIDR notation
;      localnet=169.254.0.0/255.255.0.0 ; Zero conf local network
;
; + the "externally visible" address and port number to be used when talking
;   to a host outside the NAT. This information is derived by one of the
;   following (mutually exclusive) config file parameters:
;
;   a. "externip = hostname[:port]" specifies a static address[:port] to
;      be used in SIP and SDP messages.
;      The hostname is looked up only once, when [re]loading sip.conf .
;      If a port number is not present, use the "bindport" value (which is
;      not guaranteed to work correctly, because a NAT box might remap the
;      port number as well as the address).
;      This approach can be useful if you have a NAT device where you can
;      configure the mapping statically. Examples:
;
;	externip = 12.34.56.78		; use this address.
;	externip = 12.34.56.78:9900	; use this address and port.
;	externip = mynat.my.org:12600	; Public address of my nat box.
;
;   b. "externhost = hostname[:port]" is similar to "externip" except
;      that the hostname is looked up every "externrefresh" seconds
;      (default 10s). This can be useful when your NAT device lets you choose
;      the port mapping, but the IP address is dynamic.
;      Beware, you might suffer from service disruption when the name server
;      resolution fails. Examples:
;
;	externhost=foo.dyndns.net	; refreshed periodically
;	externrefresh=180		; change the refresh interval
;
;   c. "stunaddr = stun.server[:port]" queries the STUN server specified
;      as an argument to obtain the external address/port.
;      Queries are also sent periodically every "externrefresh" seconds
;      (as a side effect, sending the query also acts as a keepalive for
;      the state entry on the nat box):
;
;	stunaddr = foo.stun.com:3478
;	externrefresh = 15
;
;   Note that at the moment all these mechanism work only for the SIP socket.
;   The IP address discovered with externip/externhost/STUN is reused for
;   media sessions as well, but the port numbers are not remapped so you
;   may still experience problems.
;
; NOTE 1: in some cases, NAT boxes will use different port numbers in
; the internal<->external mapping. In these cases, the "externip" and
; "externhost" might not help you configure addresses properly, and you
; really need to use STUN.
;
; NOTE 2: when using "externip" or "externhost", the address part is
; also used as the external address for media sessions.
; If you use "stunaddr", STUN queries will be sent to the same server
; also from media sockets, and this should permit a correct mapping of
; the port numbers as well.
;
; In addition to the above, Asterisk has an additional "nat" parameter to
; address NAT-related issues in incoming SIP or media sessions.
; In particular, depending on the 'nat= ' settings described below, Asterisk
; may override the address/port information specified in the SIP/SDP messages,
; and use the information (sender address) supplied by the network stack instead.
; However, this is only useful if the external traffic can reach us.
; The following settings are allowed (both globally and in individual sections):
;
;	nat = no		; default. Use NAT mode only according to RFC3581 (;rport)
;	nat = yes		; Always ignore info and assume NAT
;	nat = never		; Never attempt NAT mode or RFC3581 support
;	nat = route		; route = Assume NAT, don't send rport 
;				; (work around more UNIDEN bugs)

;----------------------------------- MEDIA HANDLING --------------------------------
; By default, Asterisk tries to re-invite the audio to an optimal path. If there's
; no reason for Asterisk to stay in the media path, the media will be redirected.
; This does not really work with in the case where Asterisk is outside and have
; clients on the inside of a NAT. In that case, you want to set canreinvite=nonat
;
;canreinvite=yes		; Asterisk by default tries to redirect the
				; RTP media stream (audio) to go directly from
				; the caller to the callee.  Some devices do not
				; support this (especially if one of them is behind a NAT).
				; The default setting is YES. If you have all clients
				; behind a NAT, or for some other reason wants Asterisk to
				; stay in the audio path, you may want to turn this off.

				; This setting also affect direct RTP
				; at call setup (a new feature in 1.4 - setting up the
				; call directly between the endpoints instead of sending
				; a re-INVITE).

;directrtpsetup=yes		; Enable the new experimental direct RTP setup. This sets up
				; the call directly with media peer-2-peer without re-invites.
				; Will not work for video and cases where the callee sends 
				; RTP payloads and fmtp headers in the 200 OK that does not match the
				; callers INVITE. This will also fail if canreinvite is enabled when
				; the device is actually behind NAT.

;canreinvite=nonat		; An additional option is to allow media path redirection
				; (reinvite) but only when the peer where the media is being
				; sent is known to not be behind a NAT (as the RTP core can
				; determine it based on the apparent IP address the media
				; arrives from).

;canreinvite=update		; Yet a third option... use UPDATE for media path redirection,
				; instead of INVITE. This can be combined with 'nonat', as
				; 'canreinvite=update,nonat'. It implies 'yes'.

;----------------------------------------- REALTIME SUPPORT ------------------------
; For additional information on ARA, the Asterisk Realtime Architecture,
; please read realtime.txt and extconfig.txt in the /doc directory of the
; source code.
;
;rtcachefriends=yes		; Cache realtime friends by adding them to the internal list
				; just like friends added from the config file only on a
				; as-needed basis? (yes|no)

;rtsavesysname=yes		; Save systemname in realtime database at registration
				; Default= no

;rtupdate=yes			; Send registry updates to database using realtime? (yes|no)
				; If set to yes, when a SIP UA registers successfully, the ip address,
				; the origination port, the registration period, and the username of
				; the UA will be set to database via realtime. 
				; If not present, defaults to 'yes'.
;rtautoclear=yes		; Auto-Expire friends created on the fly on the same schedule
				; as if it had just registered? (yes|no|<seconds>)
				; If set to yes, when the registration expires, the friend will
				; vanish from the configuration until requested again. If set
				; to an integer, friends expire within this number of seconds
				; instead of the registration interval.

;ignoreregexpire=yes		; Enabling this setting has two functions:
				;
				; For non-realtime peers, when their registration expires, the
				; information will _not_ be removed from memory or the Asterisk database
				; if you attempt to place a call to the peer, the existing information
				; will be used in spite of it having expired
				;
				; For realtime peers, when the peer is retrieved from realtime storage,
				; the registration information will be used regardless of whether
				; it has expired or not; if it expires while the realtime peer 
				; is still in memory (due to caching or other reasons), the 
				; information will not be removed from realtime storage

;----------------------------------------- SIP DOMAIN SUPPORT ------------------------
; Incoming INVITE and REFER messages can be matched against a list of 'allowed'
; domains, each of which can direct the call to a specific context if desired.
; By default, all domains are accepted and sent to the default context or the
; context associated with the user/peer placing the call.
; REGISTER to non-local domains will be automatically denied if a domain
; list is configured.
;
; Domains can be specified using:
; domain=<domain>[,<context>]
; Examples:
; domain=myasterisk.dom
; domain=customer.com,customer-context
;
; In addition, all the 'default' domains associated with a server should be
; added if incoming request filtering is desired.
; autodomain=yes
;
; To disallow requests for domains not serviced by this server:
; allowexternaldomains=no

;domain=mydomain.tld,mydomain-incoming
				; Add domain and configure incoming context
				; for external calls to this domain
;domain=1.2.3.4			; Add IP address as local domain
				; You can have several "domain" settings
;allowexternaldomains=no	; Disable INVITE and REFER to non-local domains
				; Default is yes
;autodomain=yes			; Turn this on to have Asterisk add local host
				; name and local IP to domain list.

; fromdomain=mydomain.tld 	; When making outbound SIP INVITEs to
                          	; non-peers, use your primary domain "identity"
                          	; for From: headers instead of just your IP
                          	; address. This is to be polite and
                          	; it may be a mandatory requirement for some
                          	; destinations which do not have a prior
                          	; account relationship with your server. 

;------------------------------ JITTER BUFFER CONFIGURATION --------------------------
; jbenable = yes              ; Enables the use of a jitterbuffer on the receiving side of a
                              ; SIP channel. Defaults to "no". An enabled jitterbuffer will
                              ; be used only if the sending side can create and the receiving
                              ; side can not accept jitter. The SIP channel can accept jitter,
                              ; thus a jitterbuffer on the receive SIP side will be used only
                              ; if it is forced and enabled.

; jbforce = no                ; Forces the use of a jitterbuffer on the receive side of a SIP
                              ; channel. Defaults to "no".

; jbmaxsize = 200             ; Max length of the jitterbuffer in milliseconds.

; jbresyncthreshold = 1000    ; Jump in the frame timestamps over which the jitterbuffer is
                              ; resynchronized. Useful to improve the quality of the voice, with
                              ; big jumps in/broken timestamps, usually sent from exotic devices
                              ; and programs. Defaults to 1000.

; jbimpl = fixed              ; Jitterbuffer implementation, used on the receiving side of a SIP
                              ; channel. Two implementations are currently available - "fixed"
                              ; (with size always equals to jbmaxsize) and "adaptive" (with
                              ; variable size, actually the new jb of IAX2). Defaults to fixed.

; jblog = no                  ; Enables jitterbuffer frame logging. Defaults to "no".
;-----------------------------------------------------------------------------------

[authentication]
; Global credentials for outbound calls, i.e. when a proxy challenges your
; Asterisk server for authentication. These credentials override
; any credentials in peer/register definition if realm is matched.
;
; This way, Asterisk can authenticate for outbound calls to other
; realms. We match realm on the proxy challenge and pick an set of 
; credentials from this list
; Syntax:
;	auth = <user>:<secret>@<realm>
;	auth = <user>#<md5secret>@<realm>
; Example:
;auth=mark:topsecret@digium.com
; 
; You may also add auth= statements to [peer] definitions 
; Peer auth= override all other authentication settings if we match on realm

;------------------------------------------------------------------------------
; Users and peers have different settings available. Friends have all settings,
; since a friend is both a peer and a user
;
; User config options:        Peer configuration:
; --------------------        -------------------
; context                     context
; callingpres                 callingpres
; permit                      permit
; deny                        deny
; secret                      secret
; md5secret                   md5secret
; transport                   transport
; dtmfmode                    dtmfmode
; canreinvite                 canreinvite
; nat                         nat
; callgroup                   callgroup
; pickupgroup                 pickupgroup
; language                    language
; allow                       allow
; disallow                    disallow
; insecure                    insecure
; trustrpid                   trustrpid
; progressinband              progressinband
; promiscredir                promiscredir
; useclientcode               useclientcode
; accountcode                 accountcode
; setvar                      setvar
; callerid		      callerid
; amaflags		      amaflags
; call-limit		      call-limit	(deprecated)
; callcounter                 callcounter
; allowoverlap		      allowoverlap
; allowsubscribe	      allowsubscribe
; allowtransfer	      	      allowtransfer
; subscribecontext	      subscribecontext
; videosupport		      videosupport
; maxcallbitrate	      maxcallbitrate
; rfc2833compensate           mailbox
; session-timers              busylevel
; session-expires            
; session-minse               template
; session-refresher           fromdomain
; t38pt_usertpsource          regexten
;                             fromuser
;                             host
;                             port
;                             qualify
;                             defaultip
;                             defaultuser
;                             rtptimeout
;                             rtpholdtimeout
;                             sendrpid
;                             outboundproxy
;                             rfc2833compensate
;                             callbackextension
;                             registertrying
;                             session-timers
;                             session-expires
;                             session-minse
;                             session-refresher
;                             timert1
;                             timerb
;                             qualifyfreq
;                             t38pt_usertpsource

;[sip_proxy]
; For incoming calls only. Example: FWD (Free World Dialup)
; We match on IP address of the proxy for incoming calls 
; since we can not match on username (caller id)
;type=peer
;context=from-fwd
;host=fwd.pulver.com

;[sip_proxy-out]
;type=peer          			; we only want to call out, not be called
;secret=guessit
;defaultuser=yourusername		; Authentication user for outbound proxies
;fromuser=yourusername			; Many SIP providers require this!
;fromdomain=provider.sip.domain	
;host=box.provider.com
;transport=udp,tcp		    ; This sets the transport type to udp for outgoing, and will
;                           ;   accept both tcp and udp. Default is udp. The first transport
;                           ;   listed will always be used for outgoing connections.
;usereqphone=yes			; This provider requires ";user=phone" on URI
;callcounter=yes			; Enable call counter
;busylevel=2				; Signal busy at 2 or more calls
;outboundproxy=proxy.provider.domain	; send outbound signaling to this proxy, not directly to the peer
;port=80				; The port number we want to connect to on the remote side
					; Also used as "defaultport" in combination with "defaultip" settings

;--- sample definition for a provider
;[provider1]
;type=peer
;host=sip.provider1.com
;fromuser=4015552299		; how your provider knows you
;secret=youwillneverguessit
;callbackextension=123		; Register with this server and require calls coming back to this extension
;transport=udp,tcp		    ; This sets the transport type to udp for outgoing, and will
;                           ;   accept both tcp and udp. Default is udp. The first transport
;                           ;   listed will always be used for outgoing connections.

;------------------------------------------------------------------------------
; Definitions of locally connected SIP devices
;
; type = user	a device that authenticates to us by "from" field to place calls
; type = peer	a device we place calls to or that calls us and we match by host
; type = friend two configurations (peer+user) in one
;
; For device names, we recommend using only a-z, numerics (0-9) and underscore
; 
; For local phones, type=friend works most of the time
;
; If you have one-way audio, you probably have NAT problems. 
; If Asterisk is on a public IP, and the phone is inside of a NAT device
; you will need to configure nat option for those phones.
; Also, turn on qualify=yes to keep the nat session open
;
; Because you might have a large number of similar sections, it is generally
; convenient to use templates for the common parameters, and add them
; the the various sections. Examples are below, and we can even leave
; the templates uncommented as they will not harm:

[basic-options](!)		; a template
	dtmfmode=rfc2833
	context=from-office
	type=friend

[natted-phone](!,basic-options)	; another template inheriting basic-options
	nat=yes
	canreinvite=no
	host=dynamic

[public-phone](!,basic-options)	; another template inheriting basic-options
	nat=no
	canreinvite=yes

[my-codecs](!)		; a template for my preferred codecs
	disallow=all
	allow=ilbc
	allow=g729
	allow=gsm
	allow=g723
	allow=ulaw

[ulaw-phone](!)		; and another one for ulaw-only
	disallow=all
	allow=ulaw

; and finally instantiate a few phones
;
; [2133](natted-phone,my-codecs)
;	secret = peekaboo
; [2134](natted-phone,ulaw-phone)
;	secret = not_very_secret
; [2136](public-phone,ulaw-phone)
;	secret = not_very_secret_either
; ...
;

; Standard configurations not using templates look like this:
;
;[grandstream1]
;type=friend 			
;context=from-sip		; Where to start in the dialplan when this phone calls
;callerid=John Doe <1234>	; Full caller ID, to override the phones config
				; on incoming calls to Asterisk
;host=192.168.0.23		; we have a static but private IP address
				; No registration allowed
;nat=no				; there is not NAT between phone and Asterisk
;canreinvite=yes		; allow RTP voice traffic to bypass Asterisk
;dtmfmode=info			; either RFC2833 or INFO for the BudgeTone
;call-limit=1			; permit only 1 outgoing call and 1 incoming call at a time
				; from the phone to asterisk (deprecated)
				; 1 for the explicit peer, 1 for the explicit user,
				; remember that a friend equals 1 peer and 1 user in
				; memory
				; There is no combined call counter for a "friend"
				; so there's currently no way in sip.conf to limit
				; to one inbound or outbound call per phone. Use
				; the group counters in the dial plan for that.
				;
;mailbox=1234@default		; mailbox 1234 in voicemail context "default"
;disallow=all			; need to disallow=all before we can use allow=
;allow=ulaw			; Note: In user sections the order of codecs
				; listed with allow= does NOT matter!
;allow=alaw
;allow=g723.1			; Asterisk only supports g723.1 pass-thru!
;allow=g729			; Pass-thru only unless g729 license obtained
;callingpres=allowed_passed_screen	; Set caller ID presentation
				; See README.callingpres for more information

;[xlite1]
; Turn off silence suppression in X-Lite ("Transmit Silence"=YES)!
; Note that Xlite sends NAT keep-alive packets, so qualify=yes is not needed
;type=friend
;regexten=1234			; When they register, create extension 1234
;callerid="Jane Smith" <5678>
;host=dynamic			; This device needs to register
;nat=yes			; X-Lite is behind a NAT router
;canreinvite=no			; Typically set to NO if behind NAT
;disallow=all
;allow=gsm			; GSM consumes far less bandwidth than ulaw
;allow=ulaw
;allow=alaw
;mailbox=1234@default,1233@default	; Subscribe to status of multiple mailboxes
;registertrying=yes             ; Send a 100 Trying when the device registers.

;[snom]
;type=friend			; Friends place calls and receive calls
;context=from-sip		; Context for incoming calls from this user
;secret=blah
;subscribecontext=localextensions	; Only allow SUBSCRIBE for local extensions
;language=de			; Use German prompts for this user 
;host=dynamic			; This peer register with us
;dtmfmode=inband		; Choices are inband, rfc2833, or info
;defaultip=192.168.0.59		; IP used until peer registers
;mailbox=1234@context,2345      ; Mailbox(-es) for message waiting indicator
;subscribemwi=yes		; Only send notifications if this phone 
				; subscribes for mailbox notification
;vmexten=voicemail		; dialplan extension to reach mailbox 
				; sets the Message-Account in the MWI notify message
				; defaults to global vmexten which defaults to "asterisk"
;disallow=all
;allow=ulaw			; dtmfmode=inband only works with ulaw or alaw!


;[polycom]
;type=friend			; Friends place calls and receive calls
;context=from-sip		; Context for incoming calls from this user
;secret=blahpoly
;host=dynamic			; This peer register with us
;dtmfmode=rfc2833		; Choices are inband, rfc2833, or info
;defaultuser=polly		; Username to use in INVITE until peer registers
;defaultip=192.168.40.123
				; Normally you do NOT need to set this parameter
;disallow=all
;allow=ulaw                     ; dtmfmode=inband only works with ulaw or alaw!
;progressinband=no		; Polycom phones don't work properly with "never"


;[pingtel]
;type=friend
;secret=blah
;host=dynamic
;insecure=port			; Allow matching of peer by IP address without 
				; matching port number
;insecure=invite		; Do not require authentication of incoming INVITEs
;insecure=port,invite		; (both)
;qualify=1000			; Consider it down if it's 1 second to reply
				; Helps with NAT session
				; qualify=yes uses default value
;qualifyfreq=60 ; Qualification: How often to check for the 
				; host to be up in seconds
				; Set to low value if you use low timeout for
				; NAT of UDP sessions
;
; Call group and Pickup group should be in the range from 0 to 63
;
;callgroup=1,3-4		; We are in caller groups 1,3,4
;pickupgroup=1,3-5		; We can do call pick-p for call group 1,3,4,5
;defaultip=192.168.0.60		; IP address to use if peer has not registered
;deny=0.0.0.0/0.0.0.0		; ACL: Control access to this account based on IP address
;permit=192.168.0.60/255.255.255.0

;[cisco1]
;type=friend
;secret=blah
;qualify=200			; Qualify peer is no more than 200ms away
;nat=yes			; This phone may be natted
				; Send SIP and RTP to the IP address that packet is 
				; received from instead of trusting SIP headers 
;host=dynamic			; This device registers with us
;canreinvite=no			; Asterisk by default tries to redirect the
				; RTP media stream (audio) to go directly from
				; the caller to the callee.  Some devices do not
				; support this (especially if one of them is 
				; behind a NAT).
;defaultip=192.168.0.4		; IP address to use until registration
;defaultuser=goran		; Username to use when calling this device before registration
				; Normally you do NOT need to set this parameter
;setvar=CUSTID=5678		; Channel variable to be set for all calls from this device
;setvar=ATTENDED_TRANSFER_COMPLETE_SOUND=beep ; This channel variable will cause the given audio file to be played
                                              ; upon completion of an attended transfer

;[pre14-asterisk]
;type=friend
;secret=digium
;host=dynamic
;rfc2833compensate=yes		; Compensate for pre-1.4 DTMF transmission from another Asterisk machine.
				; You must have this turned on or DTMF reception will work improperly.
;t38pt_usertpsource=yes         ; Use the source IP address of RTP as the destination IP address for UDPTL packets
                                ; if the nat option is enabled. If a single RTP packet is received Asterisk will know the
                                ; external IP address of the remote device. If port forwarding is done at the client side
                                ; then UDPTL will flow to the remote device.
