; Radio Repeater / Remote Base configuration file (for use with app_rpt)
; As of app_rpt version 0.39, 12/20/2005
;

;[000]					; Node ID of first repeater

;rxchannel = DAHDI/1			; Rx audio/signalling channel
; Note: if you use a unified interface (tx/rx on one channel), only
; specify the rxchannel and the txchannel will be assumed from the rxchannel
;txchannel = DAHDI/2			; Tx audio/signalling channel
;duplex = 2				; (Optional) set duplex operating mode
;; 0 = half duplex (telemetry and courtesy tones do not transmit)
;; 1 = semi-half duplex (telemetry and courtesy tones transmit, but not
;;    repeated audio
;; 2 = normal full-duplex mode (Default)
;; 3 = full-duplex mode, without repeated audio from main input source
;functions = functions-repeater		; DTMF function list
;; specify this for a different function list then local when on link
;;link_functions = functions-different	; DTMF function list for link
;;phone_functions = functions-phone	; (optional) different functions for 'P' mode
;;dphone_functions = functions-dphone	; (optional) different functions for 'D' mode
;;nodes = nodes-different		; (optional) different node list
;tonezone = us				; use US tones (default)
;context = default			; dialing context for phone
;callerid = "WB6NIL Repeater" <(213) 555-0123>  ; Callerid for phone calls
;idrecording = wb6nil			; id recording
;accountcode=RADIO			; account code (optional)
;funcchar = *				; function lead-in character (defaults to '*')
;endchar = #				; command mode end character (defaults to '#')
;;nobusyout=yes				; (optional) Do not busy-out reverse-patch when
					; normal patch in use
;hangtime=1000				; squelch tail hang time (in ms) (optional)
;totime=100000				; transmit time-out time (in ms) (optional)
;idtime=30000				; id interval time (in ms) (optional)
;politeid=30000				; time in milliseconds before ID timer
					; expires to try and ID in the tail.
					; (optional, default is 30000).
;idtalkover=|iwb6nil/rpt		; Talkover ID (optional) default is none
;unlinkedct=ct2				; unlinked courtesy tone (optional) default is none

;; The tailmessagetime,tailsquashedtime, and tailmessages need to be set
;; to support tail messages. They can be omitted otherwise.
;tailmessagetime=300000			; Play a tail message every 5 mins
;tailsquashedtime=30000			; If squashed by another user,
;;					  try again after 30 seconds
;tailmessages=msg1,msg2,msg3		;list of messages to be played for tail message

; The default values for hangtime, time-out time, and id interval time are
; 5 seconds (5000 ms),  3 minutes (180000 ms), and 5 minutes (300000 ms)
; respectively

;[001]					; Node ID of first repeater

;rxchannel = DAHDI/3			; Rx audio/signalling channel
; Note: if you use a unified interface (tx/rx on one channel), only
; specify the rxchannel and the txchannel will be assumed from the rxchannel
;txchannel = DAHDI/4			; Tx audio/signalling channel
;functions = functions-repeater		; DTMF function list
;; specify this for a different function list then local when on link
;;link_functions = functions-different	; DTMF function list for link
;;phone_functions = functions-phone	; (optional) different functions for 'P' mode
;;dphone_functions = functions-dphone	; (optional) different functions for 'D' mode
;;nodes = nodes-different		; (optional) different node list
;tonezone = us				; use US tones (default)
;context = default			; dialing context for phone
;callerid = "WB6NIL Repeater" <(213) 555-0123>  ; Callerid for phone calls
;idrecording = wb6nil			; id recording
;accountcode=RADIO			; account code (optional)
;funcchar = *				; function lead-in character (defaults to '*')
;endchar = #				; command mode end character (defaults to '#')
;;nobusyout=yes				; (optional) Do not busy-out reverse-patch when
					; normal patch in use
;hangtime=1000				; squelch tail hang time (in ms) (optional)
;totime=100000				; transmit time-out time (in ms) (optional)
;idtime=30000				; id interval time (in ms) (optional)
;politeid=30000				; time in milliseconds before ID timer
					; expires to try and ID in the tail.
					; (optional, default is 30000).
;idtalkover=|iwb6nil/rpt		; Talkover ID (optional) default is none
;unlinkedct=ct2				; unlinked courtesy tone (optional) default is none

;[002]					; Node ID of remote base

;rxchannel = DAHDI/5			; Rx audio/signalling channel
; Note: if you use a unified interface (tx/rx on one channel), only
; specify the rxchannel and the txchannel will be assumed from the rxchannel
;txchannel = DAHDI/6			; Tx audio/signalling channel
;functions = functions-remote
;remote = ft897				; Set remote=y for dumb remote or
					; remote=ft897 for Yaesu FT-897 or
					; remote=rbi for Doug Hall RBI1
;iobase = 0x378				; Specify IO port for parallel port (optional)

;[functions-repeater]
;1=ilink,1				; Specific link disconnect
;2=ilink,2				; Specific Link connect -  monitor only
;3=ilink,3				; Specific Link connect - transceive
;4=ilink,4				; Enter command mode on a specific link
;7=ilink,5				; Link status
;;XX=ilink,6				; Disconnect all links (not used here)

;80=status,1				; System info
;81=status,2				; Time
;82=status,3				; app_rpt.c Version

;6=autopatchup				; Autopatch up
;0=autopatchdn				; Autopatch down

;90=cop,1				; System warm boot
;91=cop,2				; System enable
;92=cop,3				; System disable

;[functions-remote]

;0=remote,1				; Retrieve Memory
;1=remote,2				; Set freq.
;2=remote,3				; Set Rx PL tone.
;40=remote,100				; Rx PL off
;41=remote,101				; Rx PL on
;42=remote,102				; Tx PL off
;43=remote,103				; Tx PL on
;44=remote,104				; Low Pwr
;45=remote,105				; Med Pwr
;46=remote,106				; Hi Pwr
;5=remote,5				; Status

;[telemetry]

; Telemetry entries are shared across all repeaters
; Can be a tone sequence, morse string, or a file
;
; |t - Tone escape sequence
;
; Tone sequences consist of 1 or more 4-tuple entries (freq1, freq2, duration, amplitude)
; Single frequencies are created by setting freq1 or freq2 to zero.
;
; |m - Morse escape sequence
;
; Sends Morse code at the telemetry amplitude and telemetry frequency as defined in the
; [morse] section.
;
; Follow with an alphanumeric string
;
; |i - Morse ID escape sequence
;
; Sends Morse code at the ID amplitude and ID frequency as defined in the
; [morse] section.
;
; Follow with an alphanumeric string


;ct1=|t(350,0,100,2048)(500,0,100,2048)(660,0,100,2048)
;ct2=|t(660,880,150,2048)
;ct3=|t(440,0,150,2048)
;ct4=|t(550,0,150,2048)
;ct5=|t(660,0,150,2048)
;ct6=|t(880,0,150,2048)
;ct7=|t(660,440,150,2048)
;ct8=|t(700,1100,150,2048)
;remotetx=|t(2000,0,75,2048)(0,0,75,0)(1600,0,75,2048);
;remotemon=|t(1600,0,75,2048)
;cmdmode=|t(900,903,200,2048)
;functcomplete=|t(1000,0,100,2048)(0,0,100,0)(1000,0,100,2048)


;[morse]

;speed=20		; Approximate speed in WPM
;frequency=800		; Morse Telemetry Frequency
;amplitude=4096		; Morse Telemetry Amplitude
;idfrequency=330		; Morse ID Frequency
;idamplitude=2048	; Morse ID Amplitude

;[nodes]

;000 = context_A@foo.bar.com/1234,foo.bar.com
;001 = context_B@baz.waldo.com/4321,baz.waldo.com
;002 = context_C@pepper.salt.com/5678,pepper.salt.com,y  ; this is a remote

;of course, you can also specify these with domain names, but why rely
;on DNS working unnecessarily?

;[memory]

;; this example gives you 146.460, simplex, 100.0 HZ PL, hi-power, transmit PL
;00 = 146.460,100.0,sht
;; this example gives you 146.940, minus offset, 100.0 HZ PL, low-power, no PL
;01 = 146.940,100.0,-l

; The format for these entries is:  Receive-Freq,Receive-PL,Attrbutes
;     Attributes: l=low power, m=medium power, h=high power, -=minus offset,
;	s=simplex, +=plus offset, t=tx PL enable, r=rx PL enable

